Transfer Direction (TD)

Transfer Count (TC)

General Register 0 (G0)

General Register 1 (G1)

Enable

Signals(N)

Control Sequencer

Data In

Address In

Program Counter (PC)

Control (C)

Register Read Ports

Register Write Port

Transfer Source (TS)

Instruction Prefetch

Instruction Buffer (IB) des src func

data

Data Manipulations Shifter

ALU + - & | ~

Address Out

Data Out